BIOS Update SOP

下載檔案並檢查SHA-256碼的正確性後, 將檔案解直接壓縮至USB隨身碟的根目錄
 (此隨身碟需格式化為FAT32不可開機模式)
1.	Power up the device while pressing the [Del] button repeatedly in rapid succession.
2.	If a password prompt is shown, enter the BIOS password.
3.	Select  Setup Utility.
4.	Select the Boot tab.
5.	Set USB Boot to <ENABLED>.
6.	Save the settings and exit.
7.	Connect the USB stick to the device.
8.	Reboot the device while pressing the [Del] button repeatedly in rapid succession.
9.	Select Boot Manager.
10.	Select the USB stick as the boot medium and press Enter.
11.	The BIOS will be flashed automatically. After the update is completed, the system will automatically reboot.
12.	Pressing the [Del] button repeatedly in rapid succession.
13.	Select  Setup Utility.
14.	Pressing [F9] to Check whether the BIOS version matches the downloaded version. 
